PDP-11 simulator V3.6-1
sim> set cpu 11/93
sim> set cpu 4m
Disabling CR
Disabling RK
Disabling HK
Disabling TM
sim> set rq0 rd54
sim> att rq0 rstsv9.dsk
RQ: creating new file
sim> set ts enable
sim> set ts locked
sim> att ts -f tpc rsts_v9_1_install.tap
sim> boo ts

Enabling only console, disks, and tapes.


RSTS V9.1 (MS0) INIT V9.1-05

Current date <DD-MMM-YY>? 22-OCT-99
Current time <HH:MM AM/PM>? 4:28


Installing RSTS on a new system disk? <Yes> 

22-Oct-99 04:28 AM

Disk? DU0
Pack ID? RSTSV9
Pack cluster size <8>? 
MFD cluster size <16>? 
SATT.SYS base <19448>? 
Pre-extend directories <NO>? 
PUB, PRI, or SYS <SYS>? 
[1,1] cluster size <16>? 
[1,2] cluster size <16>? 
[1,1] and [1,2] account base <19448>? 
Date last modified <YES>? 
New files first <NO>? 
Read-only <NO>? 
Patterns <3>? 
Proceed (Y or N)? Y

Pattern 3

Pattern 2

Pattern 1

Copying required system files

Enabling only console, disks, and tapes.


RSTS V9.1 (DU0) INIT V9.1-05

22-Oct-99 04:28 AM


Start timesharing? <Yes> 
  Starting SYSGEN.SIL . . .
  Rebooting . . .




RSTS V9.1 (DU0) INIT V9.1-05

22-Oct-99 04:28 AM

Creating SWAP.SYS file with minimum size of 128 blocks

  Memory allocation table:

     0K: 00000000 - 00433777 (  71K) : EXEC
    71K: 00434000 - 14657777 (1573K) : USER
  1644K: 14660000 - 16777777 ( 276K) : XBUF


Creating CRASH.SYS file with minimum size of 1224 blocks

12 devices disabled


Do you want to perform an installation or an update? <installation> 

Please mount the RSTS/E Installation media and enter the name
and unit number of the device.
Valid device types are: 'MM', 'MS', 'MT', 'MU', 'DM' or 'DL'

Installation device: MS:

Restoring required _SY0:[0,1] components


Deleting all global symbols



22-Oct-99 04:28 AM


    Beginning of the RSTS/E Software Installation Procedure

Type '?' for help
Type '^' to go back to the previous question
Type CTRL/Z to return to the beginning of the present section

  * Starting dialogue phase *


Are you ready to proceed? <yes> 

Please enter the name and unit number of the disk to
which you want to install the software. This disk
should be physically mounted and write-enabled.

Target disk? <_SY:> : 

Restoring required _SY:[1,2] components

Assigning system logicals

    ** Starting Monitor Section **


Do you want to install the RSTS/E monitor? <yes> 

Restoring required SYSGEN components

Use template monitor ?          <N >    

New Monitor name ?              <RSTS>  

Accept defaults ?               <N >    


Now you must specify the  hardware  con-
figuration  on  which this RSTS/E system
will run.


The following questions  deal  with  the
numbers and types of terminal interfaces
on the system.

Accept Terminal defaults ?      <N >    

DL11A compatible lines ?        <01>    

DL11C, DL11D's ?                <00>    

DL11E,DLV11E's ?                <00>    

DJ11's ?                        <00>    

DH11's ?                        <00>    

DZ11/DZV11/DZQ11's ?            <04>    

DZV11/DZQ11 unit 00 lines enabled ?     <04>    

DZV11/DZQ11 unit 01 lines enabled ?     <04>    

DZV11/DZQ11 unit 02 lines enabled ?     <04>    

DZV11/DZQ11 unit 03 lines enabled ?     <04>    

Dataset support for DZV11/DZQ11's ?     <N >    

DHV11's ?                       <04>    

DHV11 unit 00 lines enabled ?   <08>    

DHV11 unit 01 lines enabled ?   <08>    

DHV11 unit 02 lines enabled ?   <08>    

DHV11 unit 03 lines enabled ?   <08>    

Dataset support for DHV11's ?   <N >    

Pseudo keyboards ?              <04>    

Multi-terminal service ?        <Y >    

Echo control ?                  <Y >    

One-line status report ?        <Y >    

FMS-11 support ?                <N >    

Multiple private delimiters ?   <N >    


The following questions deal  with  the
numbers and kinds of disk units on this
system.

Accept Disk defaults ?          <N >    

RK05's ?                        <00>    

RL01/RL02's ?                   <04>    

Overlapped seek ?               <Y >    

RK06/RK07's ?                   <00>    

RP02/RP03's ?                   <00>    

Disks on DR controller ?        <08>    

Overlapped seek ?               <Y >    

Disks on DB controller ?        <00>    

MSCP disks ?                    <04>    


The following questions  deal  with  the
peripheral   devices  attached  to  this
RSTS/E system.

Accept Peripheral defaults ?    <N >    

TU16/TE16/TU45/TU77's ?         <00>    

TU10/TE10/TS03's ?              <00>    

TS11/TK25/TSV05/TU80's ?        <01>    

TMSCP tape drives ?             <01>    

DECtapes ?                      <00>    

Printers ?                      <01>    

RX01/RX02's ?                   <08>    

CR11/CM11 card reader ?         <N >    

CD11 card reader ?              <N >    

P.T. reader / punch ?           <Y >    

DECnet network support ?        <N >    

DMC11's/DMR11's ?               <00>    

KMC11's ?                       <00>    

Extended buffering for LP ?     <Y >    

RJ2780 support ?                <N >    


The following questions  deal  with  the
capacity  and  features  of  this RSTS/E
system  provided at the system manager's
option.

Accept Software defaults ?      <N >    

Maximum jobs ?                  <25>    

Small buffers ?                 <305>   

Monitor statistics ?            <N >    

EMT Logging ?                   <N >    

    ** End of Monitor Section **


    ** Starting System Programs Section **


Do you want to install the System Program packages? <yes> 

Packages to install: ALL

The following will be installed:

     RSX
     RMS
     DAP
     PBS
     EDT
     UPDATE
     TEST
     UNSUPP
     TECO
     AUXLIB
     RESTORE
     OPSER
     SORT
     HELP
     BASIC

Proceed? <yes> 

Do you want the I&D versions of tasks? <no> 

Use resident library version of RMS? <yes> 

Use RMS resident libraries in DAP? <yes> 

Use RMS resident libraries in PBS? <yes> 

Use resident library version of EDT? <yes> 

During the build phase there will be further questions
for BASIC-PLUS and SORT/MERGE

    ** End of System Programs Section **


    ** Starting Layered Products Section **


Do you want to transfer the layered product update components
from the Installation kit? <yes> 

Product updates to transfer: ALL

The following will be transferred:

     ADE
     BP2
     COBOL
     C81
     DECDX
     DECGRAPH
     DECWORD
     DIBOL
     DIBS
     DMS500
     DTR
     FMS
     FORTRAN
     FRTRN77
     F77DBG
     INDENT
     MAIL
     MENU
     MSGROUTER
     PLXY
     PROIV
     RJ2780
     RPG
     27803780
     3271

Proceed? <yes> 

NOTE: Any files currently in the PATCH ACCOUNT will be deleted

Since some layered products may require the Update package
(from the System Programs section), it will be included.
To install a layered product please refer to the individual
layered product installation guide.

Patch account <PATCH$:> : 

    ** End of Layered Products Section **


You must now set the password for account _SY:[1,2]
New password: 
New password again, for verification: 
Password set for account _SY:[1,2]

  * End of dialogue phase *


  * Starting build phase *


Are you ready to proceed? <yes> 

22-Oct-99 04:28 AM



Do you want _SY0:SWAP1.SYS created? <yes> 

Creating _SY0:[0,1]SWAP1.SYS at 3072 blocks

Creating RSTS/E monitor

This monitor has a valid buffer count
Directory of SIL RSTS  .SIL on 22-Oct-99 at 04:29 AM

 Name   Ident    Load    Size  Transfer Total

RSTS    09.105  000000  122000  000001   21K
MVR     09.105  120000  010000  000001   23K
EMT     09.105  120000  013600  000001   26K
EM2     09.105  120000  014100  000001   29K
RSX     09.105  120000  012400  000001   32K
GEN     09.105  120000  010700  000001   34K
DSK     09.105  120000  010200  000001   36K
OPN     09.105  120000  017600  000001   40K
MCP     09.105  120000  017600  000001   44K
BBR     09.105  120000  010500  000001   46K
FIP     09.105  140000  011400  000001   48K
CRA     09.105  120000  002700  000001   49K
TER     09.105  120000  025700  000001   54K
OVR     09.105  002000  126000  000001   76K
DEFALT  09.105  001000  002000  000001   76K

Resident monitor size is 56K.  By increasing this size
with the DEFAULT option of INIT, you can get additional
small buffers.  This table shows the number and type of
small buffers you can get with each size change.

Additional              Number of buffers
K-words of      With Data Space         Without Data Space
buffer space     General   FIP           General   FIP
----------------------------------------------------------
   0K               309     18              309     18
   1K               345     46              309     82
   2K               345    110              309    102
   3K               485     34              ---    ---
   4K               521     62              ---    ---
   5K               521    126              ---    ---
   6K               521    190              ---    ---
   7K               521    254              ---    ---
   8K               521    318              ---    ---
   9K               521    382              ---    ---
   10K              521    446              ---    ---
   11K              521    494              ---    ---

If you choose to run SYSGEN again, you may specify up
to 533 small buffers for this system.  Doing so will
increase some of the buffer counts in the table.





22-Oct-99 04:29 AM

Restoring the System Library package from the Installation kit
Restoring the Error package from the Installation kit
Restoring the RSX Libraries from the Installation kit
Restoring the RSX Utilities from the Installation kit
There are no updates for the RMS-11 package
Restoring the RMS Libraries from the Installation kit
Restoring the Print/Batch Services package from the Installation kit
There are no updates for the EDT package
Restoring the Update package from the Installation kit
There are no updates for the Device Testing package
Restoring the Unsupported Utilities from the Installation kit
Restoring the TECO package from the Installation kit
Restoring the Auxiliary Libraries from the Installation kit
There are no updates for the File Restore package
There are no updates for the Opser-based Spooling package
There are no updates for the SORT/MERGE package
Restoring the Help package from the Installation kit
Restoring the BASIC-PLUS package from the Installation kit
Restoring the Resident Libraries from the Installation kit

22-Oct-99 04:29 AM

Restoring ADE update components from the Installation kit
Restoring BP2 update components from the Installation kit
Restoring COBOL update components from the Installation kit
Restoring C81 update components from the Installation kit
Restoring DECDX update components from the Installation kit
Restoring DECGRAPH update components from the Installation kit
Restoring DECWORD update components from the Installation kit
Restoring DIBOL update components from the Installation kit
Restoring DIBS update components from the Installation kit
Restoring DMS500 update components from the Installation kit
Restoring DTR update components from the Installation kit
Restoring FMS update components from the Installation kit
Restoring FORTRAN update components from the Installation kit
Restoring FRTRN77 update components from the Installation kit
Restoring F77DBG update components from the Installation kit
Restoring INDENT update components from the Installation kit
Restoring MAIL update components from the Installation kit
Restoring MENU update components from the Installation kit
Restoring MSGROUTER update components from the Installation kit
Restoring PLXY update components from the Installation kit
Restoring PROIV update components from the Installation kit
Restoring RJ2780 update components from the Installation kit
Restoring RPG update components from the Installation kit
Restoring 27803780 update components from the Installation kit
Restoring 3271 update components from the Installation kit


22-Oct-99 04:29 AM


Please mount the RSTS/E Library media and enter the
name and unit number of the device.
Valid device types are: 'MM', 'MS', 'MT', 'MU', 'DM' or 'DL'

Library device <_MS:> : 
Simulation stopped, PC: 111246 (SOB R1,111244)
sim> att ts -f tpc rsts_v9_library.tap
sim> c


Restoring the System Startup files from the Library kit
Restoring the System Library package from the Library kit
File [1,2]LOGIN .TSK not replaced
File [1,2]DIRECT.TSK not replaced
File [1,2]SYSTAT.TSK not replaced
File [1,2]SAVRES.SAV not replaced
File [1,2]TERMGR.TSK not replaced
Restoring the Error package from the Library kit
File [0,3]ERRDAT.FIL not replaced
File [0,3]MSCPER.FIL not replaced
File [0,3]ERRDIS.TSK not replaced
File [0,3]ERRDET.TSK not replaced
File [0,3]ANALY1.TSK not replaced
File [0,3]ANALY3.TSK not replaced
Restoring the RSX Libraries from the Library kit
Restoring the RSX Utilities from the Library kit
File [1,2]MAKSIL.TSK not replaced
File [1,2]TKBXX .TSK not replaced
File [1,2]TKBID .TSK not replaced
File [1,2]STKXX .TSK not replaced
File [1,2]STKID .TSK not replaced
File [1,2]PRELIN.TSK not replaced
Restoring the RMS-11 package from the Library kit
Restoring the RMS Libraries from the Library kit
File [1,1]RMSLIB.OLB not replaced
File [1,1]RMSRES.TSK not replaced
File [1,1]RMSRES.STB not replaced
File [1,1]DAPRES.TSK not replaced
File [1,1]DAPRES.STB not replaced
Restoring the Print/Batch Services package from the Library kit
File [0,6]PBSRES.TSK not replaced
File [0,6]PBSOVR.TSK not replaced
File [0,6]PBSMGS.TSK not replaced
File [0,6]PBSMGV.TSK not replaced
Restoring the EDT package from the Library kit
Restoring the Update package from the Library kit
File [0,4]UPDATE.DOC not replaced
File [0,4]BUILD .TSK not replaced
Restoring the Device Testing package from the Library kit
Restoring the Unsupported Utilities from the Library kit
File [0,9]RSTSFL.OBJ not replaced
File [0,9]RSTSFL.OLB not replaced
Restoring the TECO package from the Library kit
File [0,13]TECO  .RTS not replaced
File [0,13]TECO  .DOC not replaced
File [0,13]GEXIT .OBJ not replaced
Restoring the Auxiliary Libraries from the Library kit
File [0,14]COPY  .TSK not replaced
File [0,14]DISPLY.TSK not replaced
Restoring the File Restore package from the Library kit
Restoring the Opser-based Spooling package from the Library kit
Restoring the SORT/MERGE package from the Library kit
Restoring the Help package from the Library kit
File [0,2]DCBACK.HLP not replaced
File [0,2]DCCRAC.HLP not replaced
File [0,2]DCDELE.HLP not replaced
File [0,2]DCFORC.HLP not replaced
File [0,2]DCINMT.HLP not replaced
File [0,2]DCLOAD.HLP not replaced
File [0,2]DCMTMT.HLP not replaced
File [0,2]DCREAD.HLP not replaced
File [0,2]DCSEEN.HLP not replaced
File [0,2]DCSEJO.HLP not replaced
File [0,2]DCSESY.HLP not replaced
File [0,2]DCSHCA.HLP not replaced
File [0,2]DCSHDK.HLP not replaced
File [0,2]DCSUBM.HLP not replaced
File [0,2]DCTYPE.HLP not replaced
File [0,2]DCUNLO.HLP not replaced
File [0,2]COPHLP.HLP not replaced
File [0,2]PIPHLP.HLP not replaced
File [0,2]SYSHLP.HLP not replaced
File [0,2]COPY  .HLP not replaced
File [0,2]PIPSAV.HLP not replaced
Restoring the BASIC-PLUS package from the Library kit
File [0,12]BPLGEN.SAV not replaced
File [0,12]RTS   .OBJ not replaced
File [0,12]MA2   .OBJ not replaced
File [0,12]MA2I  .OBJ not replaced
File [0,12]MA2F  .OBJ not replaced
File [0,12]MA4   .OBJ not replaced
File [0,12]MA4F  .OBJ not replaced
File [0,12]MA4D  .OBJ not replaced
File [0,12]XL2   .OBJ not replaced
File [0,12]XL2I  .OBJ not replaced
File [0,12]XL2F  .OBJ not replaced
File [0,12]XL4   .OBJ not replaced
File [0,12]XL4F  .OBJ not replaced
File [0,12]XT2   .OBJ not replaced
File [0,12]XT2I  .OBJ not replaced
File [0,12]XT2F  .OBJ not replaced
File [0,12]XT4   .OBJ not replaced
File [0,12]XT4F  .OBJ not replaced
File [0,12]SF    .OBJ not replaced
File [0,12]IO    .OBJ not replaced
File [0,12]PU    .OBJ not replaced
File [0,12]MX    .OBJ not replaced
File [0,12]SN    .OBJ not replaced
File [0,12]DBG   .OBJ not replaced
File [0,12]VE    .OBJ not replaced
File [0,12]BASIC .COM not replaced
Restoring the Resident Libraries from the Library kit
File [0,10]RMSRES.LIB not replaced
File [0,10]RMSLBF.LIB not replaced

22-Oct-99 04:30 AM

Installing software packages

22-Oct-99 04:30 AM




Beginning of RSTS/E Basic-Plus generation.


BASIC-PLUS RTS name ?           <BASIC> 

FPP ?                           <Y >    

Math precision ?                <02>    

Log functions ?                 <Y >    

Trig functions ?                <Y >    

Print using ?                   <Y >    

Matrices ?                      <N >    

String arithmetic ?             <N >    

22-Oct-99 04:30 AM


 Installing SORT/MERGE package

*********************************************************
**     This is the beginning of the dialogue to        **
**  define the attributes of your SORT/MERGE utility.  **
*********************************************************
 
This procedure will, by default, build and install
SORT and MERGE for optimum performance.  The utility
SORT and MERGE tasks will have the following attributes:
 
    SORT  built at 32K WORDS / MERGE built at 32K WORDS
    Have ASCII as the default character collating sequence
    Process duplicate records
    Do a non-stable SORT and MERGE
    Retry 2000 times when trying to read a locked bucket
    Allow 55% of the SORT work area for SORT tree structure
    Allow 30% of the MERGE work area for MERGE data structure
    Use five (5) work files for SORT
    Use the RECORD sort process
    Sequence check the input files for MERGE
 
Additionally, the default installation will NOT build the
SORT and MERGE callable subroutines as a resident library.
 
If you want the installation to proceed using
these defaults, answer YES.  If you want to
change any of these defaults, answer NO.
 
Do you want to proceed with the default installation             <YES>? 
 
************************************************
** Your SORT AND MERGE  product will be built **
** according to the following specifications: **
************************************************
 
SORT  TASK SIZE IS 32K WORDS
MERGE TASK SIZE IS 32K WORDS
YOU HAVE THE FOLLOWING RUNTIME DEFAULTS:
    ASCII CHARACTER COLLATING SEQUENCE
    RECORDS WITH DUPLICATE KEYS PROCESSED
    NO STABLE PROCESS
    2000 LOCKED BUCKET RETRIES
    55% OF WORK AREA FOR SORT DATA STRUCTURES
    45% OF WORK AREA FOR SORT RMS DATA STRUCTURES
    30% OF WORK AREA FOR MERGE DATA STRUCTURES
    70% OF WORK AREA FOR MERGE RMS DATA STRUCTURES
    05 WORK FILES
    RECORD SORT
    SEQUENCE CHECK MERGE INPUT
NO RESIDENT LIBRARY WILL BE BUILT
 
ARE THE ABOVE DEFAULTS THE DESIRED ONES    <YES or NO>           <YES>? 
 
*****************************************************
**  This is the end of the installation dialogue.  **
**    The installation will now proceed without    **
**         further operator intervention.          **
*****************************************************

Running SORT/MERGE certification tests

22-Oct-99 04:30 AM


  * End of build phase *


    The RSTS/E Software Installation Procedure is complete


Deleting all global symbols

Deassigning system logicals

22-Oct-99 04:30 AM


System tape label default set to DOS

SY:[1,2]INSTAL.LOG is a log file of this session

$ 
